IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2018-07-20T11:20:27"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1532082027 (2018-07-20T10:20:27Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1532082027 (2018-07-20T10:20:27Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_ARDEXUKLtd_CemtAdhvs_ARDEXX77" | FLOOR | names: "NBS_ARDEXUKLtd_CemtAdhvs_ARDEXX77" | material: layers "NBS_ARDEXUKLtd_CemtAdhvs_ARDEXX77" ("NBS_ARDEXUKLtd_CemtAdhvs_ARDEXX77" 3.) | property sets: COBie

Types
  IFCSLABTYPE "NBS_ARDEXUKLtd_CemtAdhvs_ARDEXX77" | FLOOR | 1 occurrence | material: layers "NBS_ARDEXUKLtd_CemtAdhvs_ARDEXX77" ("NBS_ARDEXUKLtd_CemtAdhvs_ARDEXX77" 3.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, NBS_Data, BOS_General

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_20_31_02_12:Cementitious adhesives" (IFCTEXT)
    CodePerformance = "CE marked (EN 12004)" (IFCTEXT)
    Color = "Grey or white" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Flexible wall and floor tile adhesive" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "cpd@ardex.co.uk" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "ARDEX X 77" (IFCTEXT)
    Name = "CementitiousAdhesives_ARDEXX77_ARDEXUKLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 1 type object
    AcousticRating = "n/a" (IFCTEXT)
    Combustible = FALSE (IFCBOOLEAN)
    Finish = "n/a" (IFCTEXT)
    FireRating = "Class E" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    Material = "Fibre reinforced, portland cement-based" (IFCTEXT)
    Reference = "n/a" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    TotalThickness = 3. (IFCREAL)
  NBS_Data | properties | on 1 type object
    Application = "Flexible wall and floor tile adhesive" (IFCTEXT)
    Classification = "C2 TE S1" (IFCTEXT)
    CompressiveStrength = "n/a" (IFCTEXT)
    Coverage = "Approximately 6.3 m² at 3 mm thickness per 20 kg unit" (IFCTEXT)
    DeclarationOfPerformance = ", https://ardex.co.uk/wp-content/uploads/2017/06/declaration-performance-datasheet-x-77.pdf" (IFCTEXT)
    DryingTime = "n/a" (IFCTEXT)
    HealthAndSafety = "https://ardex.co.uk/wp-content/uploads/2017/10/5e2f3962-health-safety-x-77.pdf, https://ardex.co.uk/wp-content/uploads/2017/06/health-safety-x-77-w.pdf" (IFCTEXT)
    OpenTimeMinimum = "60 minutes" (IFCTEXT)
    TensileStrength = ">1 N/mm²" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_ARDEXUKLtd_CementitiousAdhesives_ARDEXX77" (IFCTEXT)
    ManufacturerName = "ARDEX UK Ltd" (IFCTEXT)
    ManufacturerURL = "https://ardex.co.uk" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/voa2bl2c" (IFCTEXT)
    NBSDescription = "Cementitious adhesives" (IFCTEXT)
    NBSReference = "45-50-00/325" (IFCTEXT)
    ProductInformation = "https://ardex.co.uk/product/ardex-x-77/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_20_31_02_12" (IFCTEXT)
    Uniclass2015Title = "Cementitious adhesives" (IFCTEXT)
    Uniclass2015Version = "Products v1.10" (IFCTEXT)
    Version = "2" (IFCTEXT)